Date of Issue:

07 August 2014

**SAFETY DATA SHEET**

|  |
| --- |
| **1. Substance and Source Identification** |

**Product Identifier**

**SRM Number:** 154c

**SRM Name: T**itanium Dioxide

**Other Means of Identification:** Not applicable.

**Recommended Use of This Material and Restrictions of Use**

This Standard Reference Material (SRM) is intended primarily for use in the evaluation of techniques employed in the assay of titanium dioxide in the paint and ceramic industries. A unit of SRM 154c consists of a clear glass bottle containing 90 g of titanium dioxide (TiO2) as a fine powder (<45 µm).

**Company Information**

|  |  |
| --- | --- |
| National Institute of Standards and Technology |  |
| Standard Reference Materials Program |  |
| 100 Bureau Drive, Stop 2300 |  |
| Gaithersburg, Maryland 20899-2300 |  |
|  |  |
| Telephone: 301-975-2200 | Emergency Telephone ChemTrec: |
| FAX: 301-948-3730 | 1-800-424-9300 (North America) |
| E-mail: [SRMMSDS@nist.gov](mailto:SRMMSDS@nist.gov) | +1-703-527-3887 (International) |
| Website: <http://www.nist.gov/srm> |  |

|  |
| --- |
| **2. HAZARDS IDENTIFICATION** |

**Classification**

**Physical Hazard:** Not classified.

**Health Hazard:** Carcinogenicity Category 2

**Label Elements**

**Symbol**



**Signal Word**

WARNING

**Hazard Statement(s):**

H351 Suspected of causing cancer (inhalation).

**Precautionary Statement(s):**

P201 Obtain special instructions before use.

P202 Do not handle until all safety precautions have been read and understood.

P281 Use personal protective equipment as required.

P308+P313 If exposed or concerned: Get medical attention.

P405 Store locked up.

P501 Dispose of contents and container in accordance with local regulations.

**Hazards Not Otherwise Classified:** Not applicable.

**Ingredients(s) with Unknown Acute Toxicity:** Not applicable.

|  |
| --- |
| **3. COMPOSITION AND INFORMATION ON HAZARDOUS INGREDIENTS** |

**Substance:** Titanium Dioxide

**Other Designations:** Titanium oxide; titanium dioxide: TiO2; titanium peroxide; titanic oxide; brookite; rutile

Components are listed in compliance with OSHA’s 29 CFR 1910.1200; for the actual values see the NIST Certificate of Analysis.

|  |  |  |  |
| --- | --- | --- | --- |
| **Hazardous Component(s)** | **CAS Number** | **EC Number**  **(EINECS)** | **Nominal Mass Concentration  (%)** |
| Titanium Dioxide | 13463-67-7 | 236-675-5 | 100 |

|  |
| --- |
| **4. FIRST AID MEASURES** |

**Description of First Aid Measures:**

**Inhalation:** If adverse effects occur, remove to uncontaminated area. If not breathing, give artificial respiration or oxygen by qualified personnel. Seek immediate medical attention.

**Skin Contact:** Wash skin with soap and water for at least 15 minutes. Thoroughly clean and dry contaminated clothing before reuse.

**Eye Contact:** Flush eyes with water for at least 15 minutes. If necessary, seek medical attention.

**Ingestion:** If a large amount is swallowed, get medical attention.

**Most Important Symptoms/Effects, Acute and Delayed:** Irritation, cancer inhalation hazard.

**Indication of any immediate medical attention and special treatment needed, if necessary:** If any of the above symptoms are present, seek medical attention if needed.

|  |
| --- |
| **5. FIRE FIGHTING MEASURES** |

**Fire and Explosion Hazards:** Negligible fire hazard. See Section 9, “Physical and Chemical Properties” for flammability properties.

**Extinguishing Media:**

Suitable: Use extinguishing agents appropriate for surrounding fire.

Unsuitable: None listed.

**Specific Hazards Arising from the Chemical:** None listed.

**Special Protective Equipment and Precautions for Fire-Fighters:** Avoid inhalation of material or combustion byproducts. Wear full protective clothing and NIOSH approved self-contained breathing apparatus (SCBA).

**NFPA Ratings** (0 = Minimal; 1 = Slight; 2 = Moderate; 3 = Serious; 4 = Severe)

Health = 1 Fire = 0 Reactivity = 0

|  |
| --- |
| **6. ACCIDENTAL RELEASE MEASURES** |

**Personal Precautions, Protective Equipment and Emergency Procedures:** Use suitable protective equipment; see Section 8, “Exposure Controls and Personal Protection”.

**Methods and Materials for Containment and Clean up:** Collect spilled material in appropriate container for disposal. Avoid generating dust.

|  |
| --- |
| **7. HANDLING AND STORAGE** |

**Safe Handling Precautions:** Minimize dust generation. See Section 8, “Exposure Controls and Personal Protection”.

**Storage:** It is recommended that the unused portion of the powder be stored in a tightly capped container such as the original bottle or in a manner to protect against humidity. Store and handling in accordance with all current regulations and standards. Keep separated from incompatible substances (See Section 10, “Stability and Reactivity”).

|  |
| --- |
| **8. EXPOSURE CONTROLS AND PERSONAL PROTECTION** |

**Exposure Limits:**

ACGIH (TLV): 10 mg/m3 (TWA)

5000 mg/m3 (IDLH)

NIOSH (REL): No occupational exposure limits available.

OSHA (PEL): 15 mg/m3 (TWA, total dust)

**Engineering Controls:** Provide local exhaust or process enclosure ventilation system. Ensure compliance with applicable exposure limits.

**Personal Protection:** In accordance with OSHA 29 CFR 1910.132, subpart I, wear appropriate Personal Protective Equipment (PPE) to minimize exposure to this material.

**Respiratory Protection:** If workplace conditions warrant a respirator, a respiratory protection program that meets OSHA 29CFR 1910.134 must be followed. Refer to NIOSH 42 CFR 84 for applicable certified respirators.

**Eye/Face Protection:** Wear splash resistant safety goggles with a face shield. An eye wash station should be readily available near areas of use.

**Skin and Body Protection:** Personal protective equipment for the body should be selected based on the task being performed and the risks involved and should be approved by a specialist before handling this product. Chemical-resistant gloves should be worn at all times when handling chemicals.

|  |
| --- |
| **9**. **Physical and Chemical Properties** |

|  |  |
| --- | --- |
| **Descriptive Properties:** |  |
| **Appearance  (physical state, color, etc.):** | colorless, white or black, powder |
| **Molecular Formula:** | TiO2 |
| **Molar Mass (g/mol):** | 79.88 |
| **Odor:** | odorless |
| **Odor threshold:** | not available |
| **pH (solution):** | neutral (10 % suspension) |
| **Evaporation rate:** | not applicable |
| **Melting point/freezing point (ºC):** | 1825 to 1850 (3317 ºF to 3362 ºF) |
| **Relative Density**  as Specific Gravity (water = 1): | 3.84 to 4.26 |
| **Vapor Pressure (mmHg):** | not applicable |
| **Vapor Density (air = 1):** | not applicable |
| **Viscosity (cP):** | not applicable |
| **Solubility(ies):** | soluble in hot concentrated sulfuric acid, hydrofluoric acid, alkali; insoluble in water, hydrochloric acid, nitric acid, dilute sulfuric acid. |
| **Partition coefficient (n-octanol/water):** | not available |
| **Particle Size:** | <45 µm |
| **Thermal Stability Properties:** |  |
| **Autoignition Temperature (ºC):** | not applicable |
| **Thermal Decomposition (ºC):** | not available |
| **Initial boiling point and boiling range (ºC):** | 2500 to 3000 (4532 ºF to 5432 ºF) |
| **Explosive Limits, LEL (Volume %):** | not applicable |
| **Explosive Limits, UEL (Volume %):** | not applicable |
| **Flash Point (ºC):** | not applicable |
| **Flammability (solid, gas):** | not available |

|  |
| --- |
| **10. Stability and Reactivity** |

**Reactivity:** Stable at normal temperatures and pressure.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Stability:** | X | Stable |  | Unstable |

**Possible Hazardous Reactions:** None listed.

**Conditions to Avoid:** Avoid generating dust.

**Incompatible Materials:** Metals.

**Fire/Explosion Information:** See Section 5, “Fire Fighting Measures”.

**Hazardous Decomposition:** Thermal decomposition will produce oxides of titanium.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Hazardous Polymerization:** |  | Will Occur | X | Will Not Occur |

|  |
| --- |
| **11. TOXICOLOGICAL INFORMATION** |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Route of Exposure:** | X | Inhalation | X | Skin |  | Ingestion |

**Symptoms Related to the Physical, Chemical and Toxicological Characteristics:** Exposure may cause irritation; inhalation may cause cancer.

**Potential Health Effects (Acute, Chronic and Delayed):**

**Inhalation:** Acute: irritation, cough; chronic: same as acute, difficulty breathing, may cause cancer.

**Skin Contact:** Acute: no information available; chronic: irritation.

**Eye Contact:** No information available.

**Ingestion:** No information available.

**Numerical Measures of Toxicity:**

**Acute Toxicity:** Not classified.

Rat, Oral LD50: >10 000 mg/kg

**Skin Corrosion/Irritation:** Not classified.

Human, Skin intermittent (mild): 300 ug (3 d)

**Serious Eye damage/Eye irritation:** Not classified; no data available.

**Respiratory Sensitization:** Not classified; no data available.

**Skin Sensitization:** Not classified; no data available.

**Germ Cell Mutagenicity:** Not classified; no data available.

**Carcinogenicity:** Category 2.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Listed as a Carcinogen/Potential Carcinogen** | X | Yes |  | No |

Titanium dioxide is listed by IARC as Group 2B (*possibly carcinogenic to humans*). Titanium dioxide is not listed by NTP or OSHA as a carcinogen.

**Reproductive Toxicity:** Not classified; no data available.

**Specific Target Organ Toxicity, Single Exposure:** Not classified; no data available.

**Specific Target Organ Toxicity, Repeated Exposure:** Not classified; no data available.

**Aspiration Hazard:** Not classified; no data available.

|  |
| --- |
| **12. ECOLOGICAL INFORMATION** |

**Ecotoxicity Data:** No data available.

**Persistence and Degradability:** No data available.

**Bioaccumulative Potential:** No data available.

**Mobility in Soil:** No data available.

**Other Adverse effects:** No data available.

|  |
| --- |
| **13. DISPOSAL CONSIDERATIONS** |

**Waste Disposal:** Dispose of waste in accordance with all applicable federal, state, and local regulations.

|  |
| --- |
| **14. TRANSPORTATION INFORMATION** |

**U.S. DOT and IATA:** Not regulated by DOT or IATA.

|  |
| --- |
| **15. REGULATORY INFORMATION** |

**U.S. Regulations:**

CERCLA Sections 102a/103 (40 CFR 302.4): Not regulated.

SARA Title III Section 302 (40 CFR 355.30): Not regulated.

SARA Title III Section 304 (40 CFR 355.40): Not regulated.

SARA Title III Section 313 (40 CFR 372.65): Not regulated.

OSHA Process Safety (29 CFR 1910.119): Not regulated.

SARA Title III Sections 311/312 Hazardous Categories (40 CFR 370.21):

ACUTE HEALTH: No.

CHRONIC HEALTH: Yes.

FIRE: No.

REACTIVE: No.

PRESSURE: No.

**State Regulations:**

California Proposition 65: WARNING! This product contains a chemical (titanium dioxide) known to the state of California to cause cancer.

**U.S. TSCA Inventory:** Listed.

**TSCA 12(b), Export Notification:** Not listed.

**Canadian Regulations:**

WHMIS Information: Not provided for this material.

|  |
| --- |
| **16. OTHER INFORMATION** |

**Issue Date:** 07 August 2014

**Sources:** ChemAdvisor, Inc., MSDS *Titanium Dioxide*, 19 June 2014.

**Key of Acronyms:**

|  |  |  |  |
| --- | --- | --- | --- |
| ACGIH | American Conference of Governmental Industrial Hygienists | NIOSH | National Institute for Occupational Safety and Health |
| ALI | Annual Limit on Intake | NIST | National Institute of Standards and Technology |
| CAS | Chemical Abstracts Service | NRC | Nuclear Regulatory Commission |
| CEN | European Committee for Standardization | NTP | National Toxicology Program |
| CERCLA | Comprehensive Environmental Response, Compensation, and Liability Act | OSHA | Occupational Safety and Health Administration |
| CFR | Code of Federal Regulations | PEL | Permissible Exposure Limit |
| CPSU | Coal Mine Dust Personal Sample Unit | RCRA | Resource Conservation and Recovery Act |
| DOT | Department of Transportation | REL | Recommended Exposure Limit |
| EC50 | Effective Concentration, 50 % | RM | Reference Material |
| EINECS | European Inventory of Existing Commercial Chemical Substances | RQ | Reportable Quantity |
| EPCRA | Emergency Planning and Community Right-to-Know Act | RTECS | Registry of Toxic Effects of Chemical Substances |
| IARC | International Agency for Research on Cancer | SARA | Superfund Amendments and Reauthorization Act |
| IATA | International Air Transportation Agency | SCBA | Self‑Contained Breathing Apparatus |
| IDLH | Immediately Dangerous to Life and Health | SRM | Standard Reference Material |
| ISO | International Organization for Standardization | STEL | Short Term Exposure Limit |
| LC50 | Lethal Concentration, 50 % | TDLo | Toxic Dose Low |
| LD50 | Lethal Dose, 50 % | TLV | Threshold Limit Value |
| LEL | Lower Explosive Limit | TPQ | Threshold Planning Quantity |
| MSDS | Material Safety Data Sheet | TSCA | Toxic Substances Control Act |
| NFPA | National Fire Protection Association | TWA | Time Weighted Average |
| MSHA | Mine Safety and Health Administration | UEL | Upper Explosive Limit |
|  |  | WHMIS | Workplace Hazardous Materials Information System |

**Disclaimer:** Physical and chemical data contained in this SDS are provided only for use in assessing the hazardous nature of the material. The SDS was prepared carefully, using current references; however, NIST does not certify the data in the SDS. The certified values for this material are given in the NIST Certificate of Analysis.

Users of this SRM should ensure that the SDS in their possession is current. This can be accomplished by contacting the SRM Program: telephone (301) 975-2200; fax (301) 948-3730; e-mail srmmsds@nist.gov; or via the Internet at <http://www.nist.gov/srm>.