Date of Issue:

11 January 2017

**SAFETY DATA SHEET**

|  |
| --- |
| **1. Substance and Source Identification** |

**Product Identifier**

**SRM Number:** 4407H

**SRM Name:** Iodine-125 Radioactivity Standard

**Other Means of Identification:** Not applicable.

**Recommended Use of This Material and Restrictions of Use**

A unit of Standard Reference Material (SRM) 4407H consists of solution of a standardized and certified quantity of radioactive iodine-125 in a suitably stable and homogeneous matrix. The solution is contained in a 5 mL flame‑sealed borosilicate‑glass ampoule in a plastic vial in a lead shield. This SRM is intended primarily for the calibration of instruments that are used to measure radioactivity and for the monitoring of radiochemical procedures.

**Company Information**

|  |  |
| --- | --- |
| National Institute of Standards and Technology |  |
| Standard Reference Materials Program |  |
| 100 Bureau Drive, Stop 2300 |  |
| Gaithersburg, Maryland 20899-2300 |  |
|  |  |
| Telephone: 301-975-2200 | Emergency Telephone ChemTrec: |
| FAX: 301-948-3730 | 1-800-424-9300 (North America) |
| E-mail: [SRMMSDS@nist.gov](mailto:SRMMSDS@nist.gov) | +1-703-527-3887 (International) |
| Website: <http://www.nist.gov/srm> |  |

|  |
| --- |
| **2. HAZARDS IDENTIFICATION** |

**Radiological Hazard**

**Warning: THIS MATERIAL SHOULD ONLY BE USED BY PERSONS QUALIFIED TO HANDLE RADIOACTIVE MATERIAL!**

This product contains licensed radioactive material and is therefore subject to the requirements of 10 CFR Part 20 (e.g., public and occupational exposure limits, waste disposal). At a minimum, the basic radiation safety principles of time, distance, and shielding, and appropriate radiation contamination control should be practiced to avoid/minimize any external and/or internal exposure. Consult with your Radiation Safety office for your facility’s radiation safety requirements/precautions specific to the radionuclide(s) (including its activity and chemical/physical form) in this Radioactive SRM.

**SRM 4407H is a radioactive material, Iodine-125, with a total activity of approximately 750 MBq**. **Iodine-125 decays by electron capture, and during the decay process, X‑rays and gamma rays with energies from 4 keV to 36 keV are emitted. THIS SRM SHOULD ONLY BE USED BY PERSONS QUALIFIED TO HANDLE RADIOACTIVE MATERIAL!**

**Classification**

**Physical Hazard:** There are no known physical hazards associated with this material.

**Health Hazard:** Not classified.

**Label Elements**

**Symbol:** No symbol/No pictogram.

**Signal Word:** No signal word.

**Hazard Statement(s):** Not applicable.

**Precautionary Statement(s):** Not applicable.

**Hazards Not Otherwise Classified:** None.

**Ingredients(s) with Unknown Acute Toxicity:** None.

|  |
| --- |
| **3. COMPOSITION AND INFORMATION ON HAZARDOUS INGREDIENTS** |

**Substance:** Radioactive Iodine-125 solution.

**Other Designations:** Not applicable.

Components are listed in compliance with OSHA’s 29 CFR 1910.1200; for the actual values see the NIST Certificate. In addition to Iodine-125, this solution contains 0.03 % lithium hydroxide (LiOH), 0.06 % potassium iodide (KI), and 0.03 % sodium sulfite (Na2SO3) (see Certificate Table 1. Properties of SRM 4407H).

|  |  |  |  |
| --- | --- | --- | --- |
| **Components** | **CAS Number** | **EC Number**  **(EINECS)** | **Nominal Mass Concentration (%)** |
| Water | 7732-18-5 | 231-791-2 | >99 |
| Iodine – 125 | Not applicable | Not applicable | 0.0001 |

|  |
| --- |
| **4. FIRST AID MEASURES** |

**Description of First Aid Measures:**

**Inhalation:** If adverse effects occur, remove to uncontaminated area. If not breathing, give artificial respiration or oxygen by qualified personnel. Seek immediate medical attention.

**Skin Contact:** Rinse affected area with copious amounts of water followed by washing with soap and water for at least 15 minutes while removing contaminated clothing. Seek medical attention, if needed.

**Eye Contact:** Immediately flush eyes, including under the eyelids with copious amounts of water for at least 30 minutes. Seek immediate medical attention.

**Ingestion:** Contact a poison control center immediately for instructions. Wash out mouth with water, but do not induce vomiting. Seek medical aid at once, and bring the container or label.

**Most Important Symptoms/Effects, Acute and Delayed:** Not applicable.

**Indication of any immediate medical attention and special treatment needed, if necessary:** If any of the above symptoms are present, seek immediate medical attention.

|  |
| --- |
| **5. FIRE FIGHTING MEASURES** |

**Fire and Explosion Hazards:** Negligible fire hazard. See Section 9, “Physical and Chemical Properties” for flammability properties.

**Extinguishing Media:**

Suitable: Use extinguishing media appropriate to the surrounding fire.

Unsuitable: None listed.

**Specific Hazards Arising from the Chemical:** not applicable.

**Special Protective Equipment and Precautions for Fire-Fighters:** Avoid inhalation of material or combustion byproducts. Wear full protective clothing and NIOSH approved self-contained breathing apparatus (SCBA).

**NFPA Ratings:** (0 = Minimal; 1 = Slight; 2 = Moderate; 3 = Serious; 4 = Severe)

Health = 0 Fire = 0 Reactivity = 0

|  |
| --- |
| **6. ACCIDENTAL RELEASE MEASURES** |

**This material is radioactive. DO NOT touch spilled material. Immediately notify safety personnel of a spill.**

**Personal Precautions, Protective Equipment, Methods and Materials for Containment and Clean up:**

**Radiological Emergency Procedures:**

*The following is a guide for first responders. The following actions, including remediation, should be carried out by qualified individuals. In cases where a life-threatening injury occurs concurrent with personal contamination, treat the injury* ***first.***

Do not touch damaged packages or spilled material. Handle as a radioactive material spill. In addition to those actions described below, the guidelines in the 2012 Emergency Response Guidebook (ERG) provide more specific measures that should be followed.

**Spill and Leak Control:**

Alert and clear everyone from the area affected by the spill.

Take actions to limit the spread of contamination.

Summon aid.

**Damage to the Radioactive Source:**

Evacuate the immediate vicinity around the source.

Place a barrier at a safe distance from the source.

Identify area as a radiation hazard.

**Suggested Emergency Protective Equipment:**

Gloves

Footwear Covers

Outer layer or easily removed protective clothing (as situation requires)

|  |
| --- |
| **7. HANDLING AND STORAGE** |

**Safe Handling Precautions and Storage: This material is radioactive.** Store and handle in accordance with all current regulations and standards. See NRC 10 CFR 20 or state regulations. See Section 8, “Exposure Controls and Personal Protection”.

|  |
| --- |
| **8. EXPOSURE CONTROLS AND PERSONAL PROTECTION** |

**Exposure Limits:**

No established exposure limits for this solution.

**Exposure Limits: I-125**

ALIinh: 60 μCi (Thyroid) (See NRC 10 CFR 20 Appendix B)

ALIing: 40 µCi (Thyroid)

OSHA: See OSHA 29 CFR and NRC 10 CFR 20.

ACGIH: See International Commission on Radiological Protection guidelines

**Engineering Controls:** Provide local exhaust or process enclosure ventilation system. Ensure compliance with applicable exposure limits.

**Personal Protection:** In accordance with OSHA 29 CFR 1910.132, subpart I, wear appropriate Personal Protective Equipment (PPE) to minimize exposure to this material.

**Respiratory Protection:** If workplace conditions warrant a respirator, a respiratory protection program that meets OSHA 29CFR 1910.134 must be followed. Refer to NIOSH 42 CFR 84 for applicable certified respirators.

**Eye/Face Protection:** Wear splash resistant safety goggles with a face shield. An eye wash station should be readily available near areas of use.

**Skin and Body Protection:** Wear protective clothing to prevent contact with skin. Wear appropriate gloves.

|  |
| --- |
| **9. PHYSICAL AND CHEMICAL PROPERTIES** |

**NOTE:** The physical and chemical properties for this solution are reported when a measured value exists. Other values provided are for water as indicated.

|  |  |
| --- | --- |
| **Descriptive Properties:** |  |
| **Appearance (physical state, color, etc.):** | clear, colorless liquid |
| **Molecular Formula:** | >99 % H2O |
| **Molar Mass (g/mol):** | 18.02 (water) |
| **Odor:** | odorless (water) |
| **Odor threshold:** | not applicable |
| **pH:** | ~12 (measured) |
| **Evaporation rate (butyl acetate = 1):** | < 1 (water) |
| **Melting point/freezing point (ºC):** | 0 (32 ºF) (water) |
| **Relative Density (g/L)** as specific gravity (water = 1): | 1 at 20 ºC |
| **Vapor Pressure (mmHg):** | 17.5 (2 kPa) at 20 ºC (water) |
| **Vapor Density (air = 1):** | 0.62 (water vapor) |
| **Viscosity (cP):** | not available |
| **Kinematic Viscosity (mm2/s = centiStokes):** | 1.004 at 20 ºC (water) |
| **Solubility(ies):** | soluble in water and alcohols |
| **Partition coefficient (n-octanol/water):** | not applicable |
| **Thermal Stability Properties:** |  |
| **Autoignition Temperature (ºC):** | not applicable |
| **Thermal Decomposition (ºC):** | not applicable |
| **Initial boiling point and boiling range (ºC):** | 100 (212 ºF) (water) |
| **Explosive Limits, LEL (Volume %):** | not applicable |
| **Explosive Limits, UEL (Volume %):** | not applicable |
| **Flash Point (ºC):** | not applicable |
| **Flammability (solid, gas):** | not applicable |

|  |
| --- |
| **10. STABILITY AND REACTIVITY** |

**Reactivity:** This material is stable at normal temperatures and pressure.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Stability:** | X | Stable |  | Unstable |

**Possible Hazardous Reactions:** None listed.

**Conditions to Avoid:** None reported.

**Incompatible Materials:** No data available.

**Fire/Explosion Information:** See Section 5, “Fire Fighting Measures”.

**Hazardous Decomposition:** No data available.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Hazardous Polymerization:** |  | Will Occur | X | Will Not Occur |

|  |
| --- |
| **11. TOXICOLOGICAL INFORMATION** |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Route of Exposure:** | X | Inhalation | X | Skin | X | Ingestion |

**Symptoms Related to the Physical, Chemical and Toxicological Characteristics:** No adverse effects have been reported for this solution.

**Potential Health Effects (Acute, Chronic and Delayed):**

**Inhalation:** No adverse effects reported.

**Skin Contact:** No adverse effects reported.

**Eye Contact:** No adverse effects reported.

**Ingestion:** No adverse effects reported.

**Numerical Measures of Toxicity:**

**Acute Toxicity:**  Not classified; no data available this for solution.

**Skin Corrosion/Irritation:** Not classified; no data available for this solution.

**Serious Eye Damage/Eye Irritation:** Not classified; no data available for this solution.

**Respiratory Sensitization:** Not classified; no data available for this solution.

**Skin Sensitization:** Not classified; no data available for this solution.

**Germ Cell Mutagenicity:** Not classified; no data available for this solution.

**Carcinogenicity:** Not classified; no data available for this solution.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Listed as a Carcinogen/Potential Carcinogen** |  | Yes | X | No |

**Radiological Hazard**: Iodine-125

Ionizing radiation is a known carcinogen.

**Reproductive Toxicity:** Not classified; no data available for this solution.

**Specific Target Organ Toxicity, Single Exposure:** Not classified; no data available for this solution.

**Specific Target Organ Toxicity, Repeated Exposure:** Not classified; no data available for this solution.

**Aspiration Hazard:** Not classified; no data available for this solution.

|  |
| --- |
| **12. ECOLOGICAL INFORMATION** |

**Ecotoxicity Data:** No ecotoxicity data listed.

**Persistence and Degradability:** No data available.

**Bioaccumulative Potential:** No data available.

**Mobility in Soil:** No data available.

**Other Adverse Effects:** No data available.

|  |
| --- |
| **13. DISPOSAL CONSIDERATIONS** |

**Waste Disposal: This material is radioactive.** Dispose in accordance with all applicable federal, state, and local regulations for **RADIOACTIVE** materials. See NRC 10 CFR 20 subpart K.

|  |
| --- |
| **14. TRANSPORTATION INFORMATION** |

**U.S. DOT and IATA:**

**Primary Risk:** Radioactive material, Type A Package, Class 7, UN2915

**Subsidiary Risk:** Not applicable.

|  |
| --- |
| **15. REGULATORY INFORMATION** |

**U.S. Regulations:**

CERCLA Sections 102a/103 (40 CFR 302.4): Not regulated.

SARA Title III Section 302 (40 CFR 355.30): Not regulated.

SARA Title III Section 304 (40 CFR 355.40): Not regulated.

SARA Title III Section 313 (40 CFR 372.65): Not regulated.

OSHA Process Safety (29 CFR 1910.119): Not regulated.

SARA Title III Sections 311/312 Hazardous Categories (40 CFR 370.21):

ACUTE HEALTH: No.

CHRONIC HEALTH: No.

FIRE: No.

REACTIVE: No.

PRESSURE: No.

**State Regulations:**

California Proposition 65: No components are regulated.

**U.S. TSCA Inventory:** Iodine-125 islisted on inventory.

**TSCA 12(b), Export Notification:** No components are listed.

**Canadian Regulations:** WHMIS Information is not provided for this material.

|  |
| --- |
| **16. OTHER INFORMATION** |

**Issue Date:** 11 January 2017

**Sources:** ChemAdvisor, Inc., MSDS *Water,* 10 September 2014.

United States National Library of Medicine, Hazardous Substance Database (HSDB), *Iodine Radioactive*; available at <http://toxnet.nlm.nih.gov/cgi-bin/sis/htmlgen?HSDB> (accessed Jan 2017).

*CRC Handbook of Chemistry and Physics, 96th Edition*, W.M. Haynes, Ed.; CRC Press, Inc. (2015).

OSHA 29 CFR, Subpart Z, Ionizing radiation, 1910.1096.

NRC 10 CFR 20, Standards for Protection Against Radiation.

DOT 49 CFR 173, Shippers General Requirements for Shipments and Packages.

**Key of Acronyms:**

|  |  |  |  |
| --- | --- | --- | --- |
| ACGIH | American Conference of Governmental Industrial Hygienists | NIOSH | National Institute for Occupational Safety and Health |
| ALI | Annual Limit on Intake | NIST | National Institute of Standards and Technology |
| CAS | Chemical Abstracts Service | NRC | Nuclear Regulatory Commission |
| CEN | European Committee for Standardization | NTP | National Toxicology Program |
| CERCLA | Comprehensive Environmental Response, Compensation, and Liability Act | OSHA | Occupational Safety and Health Administration |
| CFR | Code of Federal Regulations | PEL | Permissible Exposure Limit |
| CPSU | Coal Mine Dust Personal Sample Unit | RCRA | Resource Conservation and Recovery Act |
| DOT | Department of Transportation | REL | Recommended Exposure Limit |
| EC50 | Effective Concentration, 50 % | RM | Reference Material |
| EINECS | European Inventory of Existing Commercial Chemical Substances | RQ | Reportable Quantity |
| EPCRA | Emergency Planning and Community Right-to-Know Act | RTECS | Registry of Toxic Effects of Chemical Substances |
| IARC | International Agency for Research on Cancer | SARA | Superfund Amendments and Reauthorization Act |
| IATA | International Air Transport Association | SCBA | Self‑Contained Breathing Apparatus |
| IDLH | Immediately Dangerous to Life and Health | SRM | Standard Reference Material |
| ISO | International Organization for Standardization | STEL | Short Term Exposure Limit |
| LC50 | Lethal Concentration, 50 % | TDLo | Toxic Dose Low |
| LD50 | Lethal Dose, 50 % | TLV | Threshold Limit Value |
| LEL | Lower Explosive Limit | TPQ | Threshold Planning Quantity |
| MSDS | Material Safety Data Sheet | TSCA | Toxic Substances Control Act |
| NFPA | National Fire Protection Association | TWA | Time Weighted Average |
| MSHA | Mine Safety and Health Administration | UEL | Upper Explosive Limit |
|  |  | WHMIS | Workplace Hazardous Materials Information System |

**Disclaimer:** Physical and chemical data contained in this SDS are provided only for use in assessing the hazardous nature of this material. The SDS was prepared carefully, using current references; however, NIST does not certify the data in the SDS. The certified values for this material are given in the NIST Certificate.

Users of this SRM should ensure that the SDS in their possession is current. This can be accomplished by contacting the SRM Program: telephone (301) 975-2200; fax (301) 948-3730; e-mail srmmsds@nist.gov; or via the Internet at http://www.nist.gov/srm.